Adafruit Industries. (2023, 10, 26). Adafruit ESP32 Feather V2. <https://cdn-learn.adafruit.com/downloads/pdf/adafruit-esp32-feather-v2.pdf>.

Bretschneider, D. E., Cannon, G. A., Holbrook, J. R., & Pashinski, D. J. (1985). Variability of subtidal current structure in a fjord estuary: Puget Sound, Washington. Journal of Geophysical Research: Oceans, 90(C6), 11949–11958. <https://doi.org/10.1029/JC090iC06p11949>.

Assendelft, R. S., & van Meerveld, H. J. I. (2019). A Low-Cost, Multi-Sensor System to Monitor Temporary Stream Dynamics in Mountainous Headwater Catchments. Sensors (Basel, Switzerland), 19(21), 4645–. https://doi.org/10.3390/s19214645

Cokelet, E. D., Stewart, R. J., & Ebbesmeyer, C. C. (1990). The annual mean transport in Puget Sound. US Department of Commerce, National Oceanic and Atmospheric Administration, Environmental Research Laboratories.

Cox, R. A. (1963). The salinity problem. Progress in Oceanography, 1, 243–261. <https://doi.org/10.1016/0079-6611(63)90006-5>.

Eriksen, C. C., Osse, T. J., Light, R. D., Wen, T., Lehman, T. W., Sabin, P. L., Ballard, J. W., & Chiodi, A. M. (2001). Seaglider: a long-range autonomous underwater vehicle for oceanographic research. IEEE Journal of Oceanic Engineering, 26(4), 424–436. <https://doi.org/10.1109/48.972073>.

Ebbesmeyer, C. C. (1984). Synthesis of current measurements in Puget Sound, Washington. Volume 3, Circulation in Puget Sound: an interpretation based on historical records of currents. NOAA Tech. Memo. NOS OMS, 5: 1–73.

Ebbesmeyer, C. C., & Barnes, C. A. (1980). Control of a fjord basin's dynamics by tidal mixing in embracing sill zones. Estuarine and Coastal Marine Science, 11(3), 311-330.

Frajka-Williams, E., Eriksen, C. C., Rhines, P. B., & Harcourt, R. R. (2011). Determining Vertical Water Velocities from Seaglider. Journal of Atmospheric and Oceanic Technology, 28(12), 1641–1656. <https://doi.org/10.1175/2011JTECHO830.1>.

Feistel, R. (2003). A new extended Gibbs thermodynamic potential of seawater. Progress in Oceanography, 58(1), 43–114. <https://doi.org/10.1016/S0079-6611(03)00088-0>.

Freescale Semiconductor, Inc. (1995). M68300 Family MC68332 User’s Manual. <https://docs.rs-online.com/b7af/0900766b806a28f4.pdf>.

Gould, J., Roemmich, D., Wijffels, S., Freeland, H., Ignaszewsky, M., Jianping, X., Pouliquen, S., Desaubies, Y., Send, U., Radhakrishnan, K., Takeuchi, K., Kim, K., Danchenkov, M., Sutton, P., King, B., Owens, B., & Riser, S. (2004). Argo profiling floats bring new era of in situ ocean observations. In Eos (Washington, D.C.) (Gould, J., et al. (2004), Argo profiling floats bring new era of in situ ocean observations, Eos Trans. AGU, 85(19), 185-191, doi:10.1029/2004EO190002., Vol. 85, Issue 19, pp. 185–191). Blackwell Publishing Ltd. <https://doi.org/10.1029/2004EO190002>.

Harrison, T. (2021). Buoyancy Controlled Float Swarms for Distributed Sensing in Coastal Waterways. ProQuest Dissertations Publishing.

Lauer, J. W., Klinger, P., O’Shea, S., & Lee, S.-Y. (2023). Development and validation of an open-source four-pole electrical conductivity, temperature, depth sensor for in situ water quality monitoring in an estuary. Environmental Monitoring and Assessment, 195(1), 221–221. <https://doi.org/10.1007/s10661-022-10493-y>.

Lyman, T. P., Elsmore, K., Gaylord, B., Byrnes, J. E. K., & Miller, L. P. (2020). Open Wave Height Logger: An open source pressure sensor data logger for wave measurement. Limnology and Oceanography, Methods, 18(7), 335–345. <https://doi.org/10.1002/lom3.10370>.

McDougall, T. J., Jackett, D. R., Millero, F. J., Pawlowicz, R., & Barker, P. M. (2012). A global algorithm for estimating Absolute Salinity. Ocean Science, 8(6), 1123–1134. https://doi.org/10.5194/os-8-1123-2012.

Ovall, B. (2019). Density structure in the outflow region of Colvos Passage: Observational analysis and model comparison [Bachelor's thesis, University of Washington]. ResearchWorks Archive. <https://digital.lib.washington.edu/researchworks/bitstream/handle/1773/45629/ovallbridgetm_3724551_56873316_Ovall-1.SeniorThesis.FinalDraft.pdf?sequence=1&isAllowed=y>.

Seim, H. E., & Gregg, M. C. (1997). The importance of aspiration and channel curvature in producing strong vertical mixing over a sill. Journal of Geophysical Research: Oceans, 102(C2), 3451–3472. <https://doi.org/10.1029/96JC03415>

Woody, C., Shih, E., Miller, J., Royer, T., Atkinson, L. P., & Moody, R. S. (2000). Measurements of Salinity in the Coastal Ocean: A Review of Requirements and Technologies. Marine Technology Society Journal, 34(2), 26–33. <https://doi.org/10.4031/MTSJ.34.2.4>.

Yang, B., Patsavas, M. C., Byrne, R. H., & Ma, J. (2014). Seawater pH measurements in the field: A DIY photometer with 0.01 unit pH accuracy. Marine Chemistry, 160, 75–81. <https://doi.org/10.1016/j.marchem.2014.01.005>.